# Change Log MAX6675

All notable changes to this project will be documented in this file.

The format is based on [Keep a Changelog](http://keepachangelog.com/)
and this project adheres to [Semantic Versioning](http://semver.org/).


## [0.3.3] - 2025-03-17
- add getCelsius() to replace getTemperature() in long term.
- add getFahrenheit() convenience wrapper.
- update examples
- update readme.md
- update unit test
- update keywords


## [0.3.2] - 2024-06-03
- add support for ARDUINO_ARCH_MBED

## [0.3.1] - 2024-04-09
- update GitHub actions
- add array example
- minor edits

## [0.3.0] - 2024-01-19
- Fix #9, improve handling SPI dependency.

----

## [0.2.0] - 2023-11-28
- refactor constructor/begin interface - breaking changes.
  - minimize conditional code. -- create SPI_CLASS macro to solve it.
- update readme.md
- update examples

----

## [0.1.3] - 2023-11-11
- update readme.md
- fix keywords.txt
- minor edits

## [0.1.2] - 2022-11-16
- add RP2040 in build-CI
- add changelog.md

## [0.1.1] - 2022-04-20
- updated documentation after tests with UNO.
- added examples

## [0.1.0] - 2022-01-11
- initial version.
