# Change Log DHT12

All notable changes to this project will be documented in this file.

The format is based on [Keep a Changelog](http://keepachangelog.com/)
and this project adheres to [Semantic Versioning](http://semver.org/).


## [0.5.0] - 2023-10-24
- simplify begin() == breaking change, see examples.
- fix examples
- add example for RP2040
- fix unit tests
- update readme.md

----

## [0.4.0] - 2023-02-09
- fix **lastRead()** initial value.
- add defaults to functions.
- update readme.md
- move code to .cpp
- update GitHub actions
- update license 2023

----

## [0.3.3] - 2022-11-01
- add changelog.md
- add rp2040 to build-CI

## [0.3.2] - 2021-12-16  
- update library.json
- update license
- add isConnected()

## [0.3.1] - 2021-10-25
- add lastRead()
- update Arduino-CI
- add badges

## [0.3.0] - 2020-12-19
- add Arduino-CI + unit test
- temperature and humidity made private

----

## [0.2.1] - 2020-06-07
- fix library.json

## [0.2.0] - 2020-04-11  
- explicit constructors, select other Wire interface, 
- #pragma once

----

## [0.1.2] - 2018-09-02 
- fix negative temperature DHT12 - issue #111

## [0.1.1] - 2017-12-19
- added ESP8266 - issue #86
- Verified by Viktor Balint

## [0.1.0] - 2017-12-11
- initial version

