# Change Log AD5620

All notable changes to this project will be documented in this file.

The format is based on [Keep a Changelog](http://keepachangelog.com/)
and this project adheres to [Semantic Versioning](http://semver.org/).


## [0.3.0] - 2025-01-20
- fix #12, redo transfer functions. Thanks to jul-brn.
- fix SPI mode, 0-> 1
- minor edits
- update readme.md

----

## [0.2.1] - 2025-01-20
- redo SW SPI, see PR #4 AD5660 library

## [0.2.0] - 2024-11-18
- fix #9 low level protocol. Send 3 bytes instead of 2.
- fix percentage functions AD5640
- update readme.md

----

## [0.1.2] - 2024-10-27
- update readme.md and comments

## [0.1.1] - 2024-10-26
- fix #3, setValue()
- add **setPowerMode()** and **getPowerMode()**
- fix #2, implement derived class **AD5640**
- update unit test
- update readme.md
- minor edits.


## [0.1.0] - 2024-10-25
- initial version, based upon AD5680

