# Change Log ADC081S

All notable changes to this project will be documented in this file.

The format is based on [Keep a Changelog](http://keepachangelog.com/)
and this project adheres to [Semantic Versioning](http://semver.org/).


## [0.3.0] - 2024-11-06
- fix #9, sync with ADC08XS
- redo low level SPI_MODE3
- update readme.md
- minor edits

----

## [0.2.2] - 2024-06-02
- add support for ARDUINO_ARCH_MBED
- minor edits

## [0.2.1] - 2024-03-03
- fix #6, add example for SPI1
- update GitHub/actions to v4 (build-CI)
- minor edits

## [0.2.0] - 2024-01-19
- fix #5, improve handling SPI dependency.
- align pin names in constructor with datasheet

----

## [0.1.2] - 2024-01-12
- add support for **ADC101S** 10 bit series
- add support for **ADC121S** 12 bit series
- update readme.md
- minor edits


## [0.1.1] - 2024-01-12
- add **void lowPower()** function
- add **void wakeUp()** function
- add **bool isLowPower()**
- add example

## [0.1.0] - 2024-01-10
- initial version.

