# Change Log HX711
All notable changes to this project will be documented in this file.

The format is based on [Keep a Changelog](http://keepachangelog.com/)
and this project adheres to [Semantic Versioning](http://semver.org/).


## [0.6.1] - 2025-06-19
- fix #65, is_ready() => set dataPin to INPUT_PULLUP
- minor edits

## [0.6.0] - 2025-04-10
- fix #60, change parameter **void calibrate_scale(float weight, uint8_t times = 10)**
- update readme.md

----

## [0.5.2] - 2024-11-18
- fix #56, update readme.md
- add parameter default for **fastProcessor**
- add **last_time_read()** to replace **last_read()** in future.
- minor edits


## [0.5.1] - 2024-11-08
- fix #54, calibration sketch should output int32_t for offset.
- update examples
- update readme.md
- minor edits

## [0.5.0] - 2024-06-17
- fix #50, bug in constructor (thanks Mathieu!)
  - refactor constructor

----

## [0.4.0] - 2024-03-02
- add fastProcessor option in **begin()** (Thanks to palmerr23)
- updated license
- updated GitHub/actions to v4

----

## [0.3.9] - 2023-11-04
- update readme.md
- minor edits

## [0.3.8] - 2023-08-26
- fix #41 #40 add example **HX_loadcell_array.ino**
  - test support array of loadcells.
- update readme.md
- add issue-count badge
- add PlatformIO badge
- minor edits

## [0.3.7] - 2023-06-27
- add example to measure noise level
- moved code to .cpp
- reorder .cpp to match .h
- removed **callibrate_scale()** (typo ll)
- add scale == 0 in **set_scale(scale)**
- changed return type to  **bool set_scale(scale)**
- add example is_ready
- add example pulse-length decoder (Morse)
- update readme.md

## [0.3.6] - 2023-03-11
- update readme.md to reference HX711_MP

## [0.3.5] - 2023-03-10
- update readme.md
- update GitHub actions
- update license 2023
- add MulitMap example
- minor edits

## [0.3.4] - 2022-11-11
- simplified changelog
- add RP2040 to build-CI
- refactored **set_gain()** to return bool to confirm valid parameter.
- add forced flag for set_gain to force a dummy read call. Default false.
- add constants for **set_gain()**
- improved unit test for **set_gain()**
- add unit test for constants.
- add delayMicroseconds(64) to power_down to enforce long enough HIGH signal.
- add power_down() power_up() cycle in **reset()**
- updated readme.md
- updated keywords.txt

## [0.3.3] - 2022-03-16
- add HX711_RAW_MODE
- update documentation

## [0.3.2] - 2022-03-16
- add example HX_set_persistent.ino. (won't work for m4)
- add CHANGELOG.md
- minor edits

## [0.3.1] - 2021-12-19
- update library.json
- license
- minor edits

## [0.3.0] - 2021-11-14
- update build-CI
- readme.md incl. badges
- fix #11 shiftIn timing

----

## [0.2.3] - 2021-05-26
- add running_average() mode

## [0.2.2] - 2021-05-10
- add read_median()
- add mode operandi
- fix typo

## [0.2.1] - 2020-12-28
- add arduino-ci
- unit test

## [0.2.0] - 2020-06-15
- add price functions
- some refactor

----

## [0.1.1] - 2019-09-09
- change long to float (reduce footprint)

## [0.1.0] - 2019-09-04
- initial version
