
Board:  ESP32 (240 Mhz)
IDE:    1.8.19

AD9833_performance.ino
AD9833_LIB_VERSION: 0.3.0


hardware:	1           (hardware SPI)
setFrequency:	48      (increased due to fix #10)
setPhase:	20
setWave:	14
writeFrequencyRegisterLSB:	23
writeFrequencyRegisterMSB:	23


hardware:	0           (software SPI)
setFrequency:	48      (increased due to fix #10)
setPhase:	15
setWave:	10
writeFrequencyRegisterLSB:	16
writeFrequencyRegisterMSB:	16


