
Board:  UNO (16 Mhz)
IDE:    1.8.19

AD9833_performance.ino
AD9833_LIB_VERSION: 0.3.0

hardware:	1            (hardware SPI)
setFrequency:	44       (increased due to fix #10)
setPhase:	24
setWave:	24
writeFrequencyRegisterLSB:	40
writeFrequencyRegisterMSB:	40


hardware:	0            (software SPI)
setFrequency:	628      (increased due to fix #10)
setPhase:	220
setWave:	220
writeFrequencyRegisterLSB:	428
writeFrequencyRegisterMSB:	432

